## Honda Multi Matic Transmission/CVT

#### Road Test (cont'd)

14-7

Position: Engine Speed rpm (min-1)

Throttle Opening | Vehicle Speed
25 mph (40 km/h) | 37 mph (60 km/h) | 62 mph (100 km/h)
Throttle position sensor voltage: 0.75 V | 1,250-1,650 | - | -
Throttle position sensor voltage: 2.0 V | 2,300-2,900 | 2,300-2,900 | 2,450-3,050
Throttle position sensor voltage: 4.5 V Fully-throttle position | 3,700-4,300 | 4,300-4,900 | 4,700-5,300

Position: Engine Speed rpm (min-1)

Throttle Opening | Vehicle Speed
25 mph (40 km/h) | 37 mph (60 km/h) | 62 mph (100 km/h)
Throttle position sensor voltage: 0.75 V | 1,800-2,400 | 2,250-2,850 | 3,300-3,900
Throttle position sensor voltage: 2.0 V | 2,600-3,200 | 3,000-3,600 | 3,800-4,400
Throttle position sensor voltage: 4.5 V Fully-throttle position | 4,100-4,700 | 5,100-5,700 | 5,500-6,100

Position: Engine Speed rpm (min-1)

Throttle Opening | Vehicle Speed
25 mph (40 km/h) | 37 mph (60 km/h) | 62 mph (100 km/h)
Throttle position sensor voltage: 0.75 V | 3,100-3,700 | 3,650-4,250 | 4,000-4,600
Throttle position sensor voltage: 2.0 V | 3,350-3,950 | 3,900-4,500 | 4,700-5,300
Throttle position sensor voltage: 4.5 V Fully-throttle position | 4,100-4,700 | 5,100-5,700 | 4,900-6,100

a a a