## SRS

#### DTC Troubleshooting (cont'd)

23-62

12. Disconnect the U1o connector (A) from the SRS unit (B).

13. Disconnect the special tool (2 ohm) from the D1i connector.
14. Check resistance between the No. 7 terminal of the U1o connector and body ground, and between the No. 16 terminal of the U1o connector and body ground. There should be 1 M ohm or more.

U1o CONNECTOR

Wire side of female terminals

Is the resistance as specified?

YES - Faulty SRS unit; replace the SRS unit (see page 23-176).

NO - Go to step 15.

15. Disconnect the cable reel from dashboard wire harness B.

16. Check resistance between the No. 7 terminal of the U1o connector and body ground, between the No. 16 terminal of the U1o connector and body ground. There should be 1 M ohm or more.

Is the resistance as specified?

YES - Replace the cable reel.

NO - Replace dashboard wire harness B.