## Interior Trim

#### Trim Removal/Installation - Seat Side and Rear Shelf Area

20-35

NOTE:

- Put on gloves to protect your hands.
- When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
- Take care not to bend or scratch the trim and panels.

Remove the trim as shown. To remove the side trim panel, remove the rear seat-back, refer to the '01 CIVIC Shop Manual, P/N 62S5A00 on this CD (see page 20-95).

Install the trim in the reverse order of removal and note these items:

- Before installing the rear shelf, remove the clips from the body and install them to the rear shelf.
- Replace any damaged clips.
- When installing the rear shelf, slip the rear seat belts and centre belt through the slits in the rear shelf.
- Make sure the high mount brake light connector is plugged in properly.

  Fastener Locations

  A : Clip, 9B : Clip, 1C : Clip, 7

  (White)

1. HIGH MOUNT BRAKE LIGHT CONNECTOR
2. HOOK
3. REAR SHELF
4. REAR CENTRE BELT
5. REAR PILLAR TRIM
6. SLIT
7. REAR SEAT BELT
8. CENTRE PILLAR UPPER TRIM
9. CAP
10. DOOR SILL TRIM
11. FRONT SEAT BELT LOWER ANCHOR BOLTS

    7/16 - 20 UNF

    32 Nm (3.3 kgf/m, 24 lbf/ft)

12. SIDE TRIM PANEL
13. HOOK
14. HOOKS
15. SLIT
16. CLIP

    (Three places)

17. HOOK
18. REAR SEAT BELT
19. SLIT