## Cylinder Head

#### Rocker Arms and Shafts Inspection (cont'd)

6-31

Camshaft Inspection

1. Inspect the rocker arm pistons (A). Push each piston manually.

   If it does not move smoothly, replace the rocker arm set.

NOTE: Apply oil to the pistons when reassembling.

NOTE: Do not rotate the camshaft during inspection.

1. Remove the rocker arm assembly (see page 6-28).

1. Put the rocker shaft holders, camshaft and camshaft holders on the cylinder head, then tighten the bolts to the specified torque.

   Specified torque:

8 mm bolts:

22 Nm (2.2 kgf/m, 16 lbf/ft)

6 mm bolts:

12 Nm (1.2 kgf/m, 8.7 lbf/ft)

6 mm bolts: (21), (22), (23)

a a a