## Seats

#### Front Seat Removal/Installation (cont'd)

20-230

4. Remove the bolts (A) securing the front seat (B).

Fastener Locations
A : Bolt, 4

5. Lift up the front seat, then detach the harness clip (A), and disconnect the seat belt switch connector (B). If equipped with a side airbag, disconnect the side airbag connector (C) and on some passenger's seat, disconnect the OPDS unit connector (D). If equipped with seat heaters, disconnect the seat heater connector (E). The passenger's seat is shown, the driver's seat is similar except it has no OPDS unit connector.

6. With the help of an assistant, carefully remove the front seat through the front door opening.
7. Install the seat in the reverse order of removal and note these items:

- Make sure each connector is plugged in properly.
- If equipped with a side airbag, reconnect the negative cable to the battery.