## Exterior Trim

#### Door Mouldings Replacement

20-117

NOTE:

- Wrap the blade of your putty knife or flat-tip screwdriver with protective tape to prevent damage to the door.
- Be careful not to pry too far or you may bend the moulding.
- Put on gloves to protect your hands.

1. Prepare to release the moulding clips from inside the vehicle.

- To remove the front door moulding, remove the front door panel (see page 20-7) and plastic cover.
- To remove the rear door moulding, remove the rear door panel (see page 20-15) and plastic cover.

2. Release the clips (A) and gently pry the front door moulding (B) or rear door moulding (C) away from the door while removing the adhesive tape (D, E).

   Fastener Locations
   A : Clip, 11

3. Install the mouldings in the reverse order of removal, and replace any damaged clips and adhesive tape.