## Power Steering

#### Hoses and Lines Replacement

17-26

Note these items during installation:

- Connect each hose to the corresponding line securely until it contacts the stop on the line. Install the clamp or adjustable clamp at the specified distance from the hose end as shown.
- Check all clamps for deterioration or deformation; replace with the clamps new ones if necessary.
- Add the recommended power steering fluid to the specified level on the reservoir and check for leaks.
- LHD type is shown, RHD type is symmetrical.

  ADJUSTABLE HOSE CLAMP (A) | HOSE CLAMP (B)

1. CYLINDER LINE FLARE NUTS

   17 Nm (1.7 kgf/m, 12 lbf/ft)

2. POWER STEERING PRESSURE SWITCH

   12 Nm (1.2 kgf/m, 8.7 lbf/ft)

3. RETURN LINE FLARE NUTS

   16 x 1.5 mm

   28 Nm (2.9 kgf/m, 21 lbf/ft)

4. FEED HOSE FLARE NUTS

   14 x 1.5 mm

   37 Nm (3.8 kgf/m, 27 lbf/ft)

5. RETURN LINE
6. RETURN HOSE
7. PUMP INLET HOSE
8. PUMP OUTLET HOSE

   11 Nm (1.1 kgf/m, 8.0 lbf/ft)