## Cylinder Head

#### Timing Belt Removal (cont'd)

6-20

11. Hold the pulley with holder handle (A) and holder attachment (B).

With P/S

With EPS

12. Remove the bolt with a 19 mm socket (C) and breaker bar.

13. Support the engine with a jack and wood block under the oil pan.
14. Remove the upper bracket.

15. Remove the grommet (A) from the upper cover and disconnect the TDC sensor connector (B).

16. Remove the upper cover (C) and lower cover (D).