## Honda Multi Matic Transmission/CVT

#### DTC Troubleshooting (cont'd)

14-305

10. Turn the ignition switch ON (II).

11. Measure the voltage between CVT speed sensor connector terminals No. 2 and No. 3.

CVT SPEED SENSOR CONNECTOR

Wire side of female terminals

Is there about 5 V?

YES - Go to step 17.

NO - Go to step 12.

12. Measure the voltage between PCM connector terminals C22 and A23 or A24.

PCM CONNECTORS

Wire side of female terminals

Is there about 5 V?

YES - Repair open in the wire between PCM connector terminal C22 and the CVT speed sensor.

NO - Check for loose terminal fit in the PCM connectors. If necessary, substitute a known-good PCM and recheck.

13. Measure the voltage between PCM connector terminal A21 and body ground.

PCM CONNECTOR A (31P)

Wire side of female terminals

Is there 4.75-5.25 V?

YES - Repair open in the wire between PCM connector terminal A21 and the CVT speed sensor.

NO - Go to step 14.

14. Turn the ignition switch OFF.
15. Disconnect PCM connector C (22P).
16. Check for continuity between PCM connector terminal A21 and body ground.

PCM CONNECTOR A (31P)

Wire side of female terminals

Is there continuity?

YES - Repair short to ground in the wire between PCM connector terminal A21 and the CVT speed sensor.

NO - Check for loose terminal fit in the PCM connectors. If necessary, substitute a known-good PCM and recheck.