## Soft Chipping Guard Primer Coat

#### Undercoating Diagram

5-27

Indicated PVC coating area.

NOTE:

- Coating thickness 0.4mm (0.16 in.) MIN.
- Front wheelhouse, rear wheelhouse and dashboard lower on the imported control area, and coating thickness 0.5 mm (0.2 in.).

  1. FRONT SIDE DAMPER
  2. DAMPER HOUSING
  3. OUTER PANEL
  4. FRONT FLOOR CENTRE CROSS-MEMBER

SECTION AA SECTION BB SECTION CC SECTION DD

SECTION EE

1. Dashboard Lower
2. Front Floor
3. Middle Floor Cross-member
4. Rear Floor Cross-member

SECTION FF

1. <Front Wheelhouse>
2. <Rear Wheelhouse>
3. OUTER PANEL
4. FUEL DOOR ADAPTOR SECTION
5. FUEL DOOR ADAPTOR
6. No Coating Area.

VIEW (Z)