## Air Conditioning

#### Refrigerant Discharge

21-94

CAUTION

- Air conditioning refrigerant or lubricant vapour can irritate your eyes, nose or throat.
- Be careful when connecting service equipment.
- Do not breathe refrigerant or vapour.

Use only a gauge set for refrigerant HFC-134a (R-134a).

If accidental system discharge occurs, ventilate work area before resuming service.

Additional health and safety information may be obtained from the refrigerant and lubricant manufacturers.

1. Connect the R-134a gauge set as shown.

THREE VALVE GAUGE:

1. LOW-PRESSURE VALVE
2. EVACUATION VALVE
3. HIGH-PRESSURE VALVE
4. HIGH-PRESSURE QUICK JOINT
5. LOW-PRESSURE QUICK JOINT

TWO VALVE GAUGE

1. LOW-PRESSURE VALVE
2. HIGH-PRESSURE VALVE
3. HIGH-PRESSURE QUICK JOINT
4. LOW-PRESSURE QUICK JOINT

1. Disconnect the centre hose of the gauge set and place the free end in a shop towel.
2. Open the evacuation valve (two valve gauge: evacuate stop valve).
3. Slowly open the high-pressure valve slightly to let refrigerant flow from the centre hose only. Do not open the valve too wide. Check the stop towel to make sure no oil is being discharged with the refrigerant.

If refrigerant is allowed to escape too fast, compressor oil will be drawn out of the system.

5. After the high-pressure gauge reading has dropped below 980 kPa (10 kgf/cm2, 140 psi), open the low side valve to discharge both high and low sides of the system.
6. Note the gauge reading and as system pressure drops, gradually open both high and low side valves fully until both gauges indicate 0 kPa (0 kgf/cm2, 0 psi).