## Intake Manifold and Exhaust System

#### Turbocharger and Exhaust Manifold Removal (cont'd)

9-6

Turbocharger and Exhaust Manifold Installation

1. Remove the exhaust pipe A (A) from the turbocharger.

1. Remove the oil feed pipe (B) and disconnect the turbocharger return hose (C) from the turbocharger (D).

1. Remove the exhaust manifold fixing nuts and remove the exhaust manifold (E).

1. Remove the turbocharger fixing nuts (A) and turbocharger exhaust pipe fixing nuts (B), then remove the turbocharger assembly (C).

1. Install the turbocharger exhaust pipe (A) with gasket to turbocharger (B) and install the turbocharger with gasket to exhaust manifold (C). Tighten fastening nuts (D) to the specified torque.

   Specified torque:

Temporary tightening 38.8 Nm (4.0 kgf/m, 29 lbf/ft)

Fully tightening 77.5 Nm (7.9 kgf/m, 57 lbf/ft)

1. Install the exhaust manifold with gasket.

a a a