## Engine Assembly

#### Engine Installation (cont'd)

5-10

1. Position the engine under the vehicle. Attach the chain hoist to the engine, then lift the engine into position in the vehicle.

Reinstall the mounting bolts/support nuts in the sequence given. Failure to follow this sequence may cause excessive noise and vibration and reduce bushing life.

1. Install the sub-frame (A). Align the reference lines (B) on the sub-frame with the bolt head centre, then tighten the bolts.

1. 10 x 1.25 mm

   59 Nm (6.0 kgf/m, 43 lbf/ft)

2. 14 x 1.5 mm

   103 Nm (10.5 kgf/m, 76 lbf/ft)

   Replace.

1. Tighten the front mount mounting bolt.

1. 12 x 1.25 mm

   64 Nm (6.5 kgf/m, 47 lbf/ft)

   Replace.

1. Tighten the rear mount mounting bolts.

1. 10 x 1.25 mm

   59 Nm (6.0 kgf/m, 43 lbf/ft)

a a a