## Seats

#### Rear Seat-back Cover Replacement - Fixed Type

20-102

NOTE:

- Take care not to tear the seams or damage the seat covers.
- Put on gloves to protect your hands.

1. Remove the seat-back (see page 20-96).
2. If equipped, remove the armrest (see page 20-98).
3. Release all the clips (A) and hook strips (B) (with armrest), and fold back the seat-back cover (C).

4. Pull back the edge of the seat-back cover (A) all the way around, and release the clips (B), then remove the seat-back cover.

5. Install the cover in the reverse order of removal, and note these items:

- To prevent wrinkles when installing a seat-back cover, make sure the material is stretched evenly over the pad before securing the hooks and clips.
- Replace any clips you removed with new ones. Install them with commercially available upholstery ring pliers.