## Automatic Transmission

#### General Troubleshooting Information (cont'd)

14-5

Codes 1 through 9 are indicated by individual short blinks. Code 10 and above are indicated by a series of long and short blinks. One long blink equals 10 short blinks. Add the long and short blinks together to determine the code. After determining the code, refer to the DTC Troubleshooting Index.

If the indicator light and the MIL (Malfunction Indicator Lamp) come on at the same time, or if a driveability problem is suspected, follow this procedure:

1. Record all fuel and emission DTCs, A/T DTCs and freeze data.
2. If there is a fuel and emissions DTC, first check the fuel and emissions system as indicated by the DTC (except for DTC 70, DTC 70 means there is one or more A/T DTCs and no problems were detected in the fuel and emissions circuit of the PCM.
3. Write down the radio station presents.
4. Reset the memory by removing the No. 6 ECU (PCM) fuse in the under-hood fuse/relay box for more than 10 seconds.
5. Drive the vehicle for several minutes at speeds over 30 mph (50 km/h) and then recheck for DTC. If the A/T DTC returns, go to the DTC Troubleshooting Index. If the DTC does not return, there was an intermittent problem within the circuit. Make sure all pins and terminals in the circuit are tight and then go to step 6.
6. Reset the radio preset stations and set the clock.