## SRS

#### DTC Troubleshooting - with Side Airbags (cont'd)

23-121

DTC 13-3: No Signal from the Left Side Impact Sensor (Without OPDS Unit Model)

1. Erase the DTC memory (see page 23-38).
2. Turn the ignition switch ON (II), and check that the SRS indicator light comes on for about 6 seconds and then goes off.

Does the SRS indicator light stay on?

YES - Go to step 3.

NO - Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failures (see page 23-38).

3. Turn the ignition switch OFF. Disconnect the battery negative cable and wait for 3 minutes.
4. Check the connection between the ILi connector and the left side impact sensor.

Is the connection OK?

YES - Go to step 5.

NO - Poor contact between the ILi connector and the left side impact sensor; reconnect or replace the left side impact sensor.

5. Disconnect the SLi and SRi connectors.

6. Disconnect the ILi connector (A) from the left side impact sensor (B).

7. Connect the special tool (Jumper) to the ILi connector.
8. Disconnect the U2o connector (A) from the SRS unit (B).