## SRS

#### DTC Troubleshooting (cont'd)

23-85

DTC 5-1, 5-2, 5-3, 5-4, 5-5, 5-8, 6-1, 6-2, 6-3, 6-4, 6-7, 6-8, 7-1, 7-2, 7-3, 8-1, 8-2, 8-3, 8-4, 8-5, 8-6, 9-1, 9-2: Internal Failure of the SRS Unit NOTE: Before troubleshooting any of these DTCs, check battery/system voltage. If voltage is low, repair the charging system before troubleshooting the SRS system.

1. Erase the DTC memory (see page 23-38).
2. Turn the ignition switch ON (II), and check that the SRS indicator light comes on for about 6 seconds and then goes off.

Does the SRS indicator light stay on?

YES - Replace the SRS unit (see page 23-176).

NO - Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failures (see page 23-38).

DTC 10-1, 10-2, 10-3, 10-4, 10-5, 10-6, 10-7: Airbags, Side Airbags and/or Seat Belt Tensioners Deployed

The SRS unit must be replaced after any airbags have deployed (see page 23-176).