## Shafts and Clutches

#### Sub-shaft Transmission Housing Needle Bearing Replacement

14-204

Special Tools Required

- Handle driver, 07749-0010000
- Driver attachment, 32 x 35 mm, 07746-0010100

1. Remove the sub-shaft transmission housing bearing (see page 14-177).
2. Remove the needle bearing stop.
3. Remove the needle bearing from the transmission housing with the special tool.

4. Install the new needle bearing in the transmission housing with the special tools and a press.

5. Install the sub-shaft transmission housing bearing (see page 14-177).