## SRS

#### DTC Troubleshooting Index (cont'd)

23-44

SIEMENS (M1), KEIHIN (M3 or M4) SRS unit (Side Airbag with OPDS Unit Model)

DTC | Detection Item | Notes
1-1 | Open or increased resistance in driver's airbag inflator | (see page 23-55)
1-3 | Short to another wire or decreased resistance in driver's airbag inflator | (see page 23-57)
1-4 | Short to power in driver's airbag inflator | (see page 23-59)
1-5 | Short to ground in driver's airbag inflator | (see page 23-61)
2-1 | Open or increased resistance in front passenger's airbag inflator | (see page 23-63)
2-3 | Short to another wire or decreased resistance in front passenger's airbag inflator | (see page 23-64)
2-4 | Short to power in front passenger's airbag inflator | (see page 23-66)
2-5 | Short to ground in front passenger's airbag inflator | (see page 23-67)
3-1 | Open or increased resistance in left side seat belt tensioner | (see page 23-69)
3-3 | Short to another wire or decreased resistance in left side seat belt tensioner | (see page 23-71)
3-4 | Short to power in left side seat belt tensioner | (see page 23-73)
3-5 | Short to ground in left side seat belt tensioner | (see page 23-75)
4-1 | Open or increased resistance in right side seat belt tensioner | (see page 23-77)
4-3 | Short to another wire or decreased resistance in right side seat belt tensioner | (see page 23-79)
4-4 | Short to power in right side seat belt tensioner | (see page 23-81)
4-5 | Short to ground in right side seat belt tensioner | (see page 23-83)
5-1 | Internal failure of SRS unit | (see page 23-85)
5-2
5-4
5-8
6-3
6-4
6-7
6-8
7-1
7-2
7-3
8-1
8-2
8-3
8-4
8-5
8-6

NOTE:

Before troubleshooting DTCs 5-1 through 8-6, check battery/system voltage. If voltage is low, repair the charging system before troubleshooting the SRS system.