## Design Specifications

#### (cont'd)

2-19

Item | Measurement | Qualification | Specification
ENGINE | Lubrication system |  | Forced, wet sump, with trochoid pump
Oil pump displacement | at 6,000 engine rpm | 36.4 l (38.5 US qt, 32.0 imp qt)/minute
Water pump displacement | at 6,000 engine rpm | 130 l (137 US qt, 114 imp qt)/minute
Fuel required | KK model | UNLEADED gasoline with 91 research octane number or higher
KB, KE, KG, KR models | Premium UNLEADED gasoline with 95 research octane number or higher
KX model | UNLEADED gasoline with 91 research octane number or higher (RON of 95 UNLEADED gasoline may also be used)
KY model | LEADED gasoline with 91 research octane number or higher (RON of 91 UNLEADED gasoline may also be used)
STARTER | Type |  | Gear reduction
Normal output |  | 1.0 kW
Hour rating |  | 30 seconds
Direction of rotation |  | Clockwise as viewed from gear end
CLUTCH | Clutch | M/T | Single plate dry, diaphragm spring
A/T | Torque converter
Clutch friction material surface area | M/T | 176 cm3 (102 sq in.)
MANUAL TRANS-MISSION | Type |  | Synchronised, 5-speed forward, 1 reverse
Primary reduction |  | Direct 1:1
Gear ratio | 1st | 3.461
2nd | 1.869
3rd | 1.241
4th | 0.969
5th | 0.805
Reverse | 3.230
Final reduction | Type | Single helical gear
Gear ratio | 4.411
AUTOMATIC TRANS-MISSION | Type |  | Electronically controlled automatic, 4-speed forward, 1 reverse
Primary reduction |  | Direct 1:1
Gear ratio | 1st | 2.722
2nd | 1.468
3rd | 0.975
4th | 0.674
Reverse | 1.955
Final reduction | Type | Single helical gear
Gear ratio | 4.357
STEERING | Type |  | Rack and pinion, with electrical power assistance/hydraulic power assistance
Overall ratio |  | 14.49
Turns, lock-to-lock |  | 2.83
Steering wheel diameter |  | 380 mm (15.0 in.)
SUSPENSION | Type |  | Strut
Rear | Double wishbone
Shock absorber | Front and rear | Telescopic, hydraulic, nitrogen gas-filled