## Seats

#### Front Seat Cover Replacement (cont'd)

20-94

Seat Cushion Cover

1. Remove the front seat (see page 20-87).
2. Remove the recline cover and centre cover, with manual height (see page 20-89), without manual height (see page 20-90).
3. With side airbag: From under the seat cushion, detach the side airbag connector clip, and on the passenger's seat, detach the OPDS unit connector clip. Release the hook springs.
4. Release the hooks (A) from both sides the seat cushion.

5. Release the seat-back cover (A) from the cushion frame spring (B), and release the hooks (C) from under the seat cushion.

6. Pull back the edge of the seat cushion cover all the way around, and release the clips (A), then remove the seat cushion cover.

7. Install the cover in the reverse order of removal, and note these items:

- To prevent wrinkles when installing a seat cushion cover, make sure the material is stretched evenly over the pad before securing the clips and hooks.
- Replace any clips you removed with new ones (A). Install them with commercially available upholstery ring pliers (B).