## Lubricants and Fluids

####

3-2

For the details of lubrication points and type of lubricants to be applied, refer to the illustrated index and various work procedures (such as Assembly/Reassembly, Replacement, Overhaul, Installation, etc.) contained in each section.

NO. | LUBRICATION POINTS | LUBRICANT
1 | Engine | Always use fuel-efficient is that says "API service SG, SH or SJ" SAE Viscosity See chart below.
2 | Transmission | Genuine Honda Manual Transmission Fluid (MTF) *1
3 | Brake system (includes ABS line) | Brake fluid DOT 3 or DOT 4 *2
4 | Clutch line | Brake fluid DOT 3 or DOT 4 *2
5 6 | Release fork Shift and select cable ends | Super High Temp Urea Grease (P/N 08798-9002)
7 | Throttle cable end (dashboard lower panel hole) | Silicon grease
8 9 10 11 12

13

14

Throttle cable end (throttle link)

Brake master cylinder pushrod

Clutch master cylinder pushrod

Shift lever

Pedal linkage

Battery terminals

Fuel filler lid

Multi-purpose grease
15 16 17 18 | Hood hinges and latch Tailgate hinges Door hinges, upper and lower Door opening detent | Honda White Lithium Grease
19 | Caliper piston boot, caliper pins and boots | Silicon grease
20 | Brake line joints (front and rear wheelhouse) | Rust preventives

Recommended Engine Oil

Engine oil viscosity for ambient temperature ranges

CAUTION Used engine oil may cause skin cancer if repeatedly left in contact with skin for prolonged periods. Although this is unlikely unless you handle used oil on a daily basis, it is sill advisable to thoroughly wash your hands with soap and water as soon as possible after handling used oil.

*1: | Always use genuine Honda Manual Transmission Fluid (MTF). Using motor oil can cause stiffer shifting because it does not contain the proper additives.
*2: | We recommend Genuine Honda Brake Fluid. Using a non-Honda brake fluid can cause corrosion and decrease the life of the system.

a a a