## Shafts and Clutches

#### Clutch Reassembly

14-211

Special Tools Required

- Clutch spring compressor set, 07LAE-PX40000
  - Clutch spring compressor attachment, 07LAE-PX40100
  - Clutch spring compressor attachment, 07HAE-PL50101
  - Clutch spring compressor bolt assembly, 07GAE-PG40200

- Snap ring pliers, 07LAC-0010100

NOTE:

- Clean all parts thoroughly in solvent or carburettor cleaner and dry them with compressed air.
- Blow out all passages.
- Apply ATF to all parts before assembly.

1. Inspect the check valve (A); if it's loose, replace the piston (B).

2. Install new O-rings (A) on the piston (B).

3. Install the piston (A) in the clutch drum (B). Apply pressure and rotate to ensure proper seating.

Lubricate the piston O-ring with ATF before installing.

NOTE: Do not pinch the O-ring by installing the piston with too much force.