## Seat Belts

#### Rear Seat Belt Replacement (cont'd)

23-9

Centre Belt and Seat Belt Buckles

1. Remove the rear seat cushion, folding type (see page 20-95), fixed type (see page 20-96).
2. Remove the centre anchor bolts (A), and remove the seat belt buckles (B).

With centre shoulder belt:

With centre lap belt:

With centre shoulder belt:

3. Remove the rear shelf, folding type (see page 20-65).
4. Remove the retractor mounting self-tapping ET screw (A) and the retractor bolt (B), then remove the centre belt (C) and retractor (D).

5. Remove the protector (A).