## Cylinder Head

#### Camshaft Inspection (cont'd)

6-21

9. Check the total runout with the camshaft supported on V-blocks.

- If the total runout of the camshaft is within the service limit, replace the cylinder head.
- If the total runout is beyond the service limit, replace the camshaft and recheck the camshaft-to-holder oil clearance. If the oil clearance is still out of tolerance, replace the cylinder head.

Camshaft Total Runout:

Standard (New):0.03 mm (0.001 in.) max.

Service Limit:0.04 mm (0.002 in.)

1. Rotate camshaft while measuring

10. Measure cam lobe height.

Cam Lobe Height Standard (New):

| INTAKE | EXHAUST
D17A2, D17A5, D17A9, engines | PRI | 38.604 mm (1.5198 in.) | 38.784 mm (1.5269 in.)
| SEC | 32.848 mm (1.2932 in.) |
D17A8 engine | 35.299 mm (1.3897 in.) | 37.281 mm (1.4678 in.)

PRI: PrimarySEC: Secondary

IN: IntakeEX: ExhaustT/B: Timing Belt