## SRS

#### Cable Reel Replacement (cont'd)

23-174

8. Disconnect the dashboard wire harness B 4P connector (A) from the cable reel 4P connector (B), then disconnect the dashboard wire harness B 5P connector (C) from the cable reel (D).

9. Release the tab (A), then remove the cable reel from the column.

Installation

1. Before installing the steering wheel, align the front wheels straight ahead.
2. Disconnect the battery negative cable and wait at least 3 minutes.
3. Set the cancel sleeve (A) so that the projections (B) are aligned vertically.

4. Carefully install the cable reel (A) on the steering column shaft. Then connect the 5P connector (B) to the cable reel, and connect the 4P connector (C) to the SRS main harness 4P connector (D).