## Seats

#### Front Seat Disassembly/Reassembly - Driver's

20-231

For some models: SRS components are located in this area. Review the SRS component locations (see page 23-24) and the precautions and procedures (see page 23-25) in the SRS section before performing repairs or service.

NOTE:

- Take care not to tear the seams or damage the seat covers.
- Put on gloves to protect your hands.
- When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.

Disassemble the seat as shown.

Reassemble the seat in the reverse order of disassembly and note these items:

- Apply multipurpose grease to the moving portion of the seat track.
- To prevent wrinkles in the seat cushion cover, stretch the material evenly over the pad.

  1. SEAT-BACK
  2. HEADREST
  3. HOOKS
  4. Release the seat cushion cover from the cushion frame spring.
  5. HOOKS
  6. HANGER SPRING

     (With side airbag)

  7. CLIP
  8. HOOKS

     (Five places)

  9. SEAT HEATER HARNESS

     (For some models)

  10. HOOK
  11. CENTRE COVER
  12. HOOKS
  13. CLIP
  14. CLIP
  15. SEAT CUSHION FRAME/SEAT TRACKS
  16. SLIDE LEVER
  17. SEAT HEATER UNIT

      (For some models)

  18. CLIP
  19. HOOK
  20. CLIP
  21. CLIP
  22. CAP
  23. HEIGHT HANDLE
  24. RECLINE KNOB
  25. CLIP
  26. RECLINE COVER
  27. HOOK
  28. SIDE AIRBAG HARNESS