## Charging System

#### Alternator Overhaul (cont'd)

4-32

12. With a hammer and commercially available tools shown, install a new rear bearing on the rotor shaft.

13. Remove the front bearing retainer plate.

14. Support the stator housing in a vice, and drive out the front bearing with a brass drift and hammer.

15. With a hammer and the special tools, install a new front bearing in the stator housing.

a a a