## Shafts and Clutches

#### Clutch Inspection

14-208

1ST CLUTCH

1. 1ST CLUTCH DRUM
2. O-RING, Replace
3. CLUTCH PISTON
4. WAVE SPRING
5. RETURN SPRING
6. SPRING RETAINER
7. SNAP RING
8. CLUTCH PLATES, 3

   Standard thickness:

   1.6 mm (0.06 in.)

9. CLUTCH DISCS, 3

   Standard thickness:

   1.94 mm (0.076 in.)

10. CLUTCH END PLATE
11. SNAP RING

3RD CLUTCH

1. SNAP RING
2. CLUTCH END PLATE
3. CLUTCH DISCS, 3

   Standard thickness:

   1.94 mm (0.076 in)

4. CLUTCH PLATES, 4

   Standard thickness:

   2.00 mm (0.079 in)

5. SNAP RING
6. SPRING RETAINER
7. RETURN SPRING
8. WAVE WASHER
9. CLUTCH PISTON
10. O-RING, Replace
11. 3RD CLUTCH DRUM