## PGM-FI System

#### MIL Circuit Troubleshooting (cont'd)

11-40

62. Check for continuity between ECM/PCM connector terminal A21 and body ground.

ECM/PCM CONNECTOR A (31P)

Wire side of female terminals

Is there continuity?

YES - Repair short in the wire between the ECM/PCM (A21) and the MAP sensor.

NO - Substitute a known-good ECM/PCM and recheck, refer to the '01 Civic Shop Manual on this CD (see page 11-313). If symptom/indication goes away, replace the original ECM/PCM.

63. Measure voltage between body ground and ECM/PCM connector terminal A20.

ECM/PCM CONNECTOR A (31P)

Wire side of female terminals

Is there about 5 V?

YES - Substitute a known-good ECM/PCM and recheck, refer to the '01 Civic Shop Manual on this CD (see page 11-313). If symptom/indication goes away, replace the original ECM/PCM.

NO - Go to step 64.

64. Turn the ignition switch OFF.
65. Disconnect the 3P connector from each of these sensors, one at a time and measure voltage between body ground and ECM/PCM connector terminal A20 with the ignition switch ON (II).

- Exhaust gas recirculation (EGR) valve position sensor
- Knock sensor
- Throttle position (TP) sensor

ECM/PCM CONNECTOR A (31P)

Wire side of female terminals

Is there about 5 V?

YES - Replace the sensor that restored about 5 V when disconnected.

NO - Go to step 66.

66. Turn the ignition switch OFF.
67. Disconnect the 3P connectors from the following sensors.

- Exhaust gas recirculation (EGR) valve position sensor
- Knock sensor
- Throttle position (TP) sensor

68. Disconnect ECM/PCM connector A (31P).