## Security System

#### Door Lock Knob Switch Test

22-262

Driver's door (4-door):

1. Remove the driver's door panel (see page 20-7).
2. Disconnect the 3P connector (A) from the actuator (B).

3. Check for continuity between the terminals in each switch position according to the table.

Passenger's door (4-door):

1. Remove the passenger's door panel (see page 20-7).
2. Disconnect the 3P connector (A) from the actuator.

3. Check for continuity between the terminals in each switch position according to the table.

Front passenger's:

Left rear:

Right rear: