## Engine Assembly

#### Engine Removal (cont'd)

5-6

16. Remove the harness clamps (A) and grommet (B), then pull the engine wire harness through the bulkhead.

RHD models:

LHD models:

17. Remove the throttle cable (A) and cruise control cable (B) by loosening the locknuts (C), then slipping the cable ends out of the accelerator linkage. Take care not to bend the cables when removing them. Always replace any kinked cable with a new one.

18. Remove the adjust plate mounting bolt (A), lock nut (B) and mounting bolt (C), then remove the power steering (P/S) pump belt (D) and pump without disconnecting the P/S hoses (P/S).