## Doors

#### Front Door Upper Seal Replacement

20-14

Front Door Side Sill Seal Replacement

NOTE:

- Take care not to scratch the door.
- Use a clip remover to remove the clips.

1. Remove these items:

- Power mirror/manual mirror, as necessary (see page 20-33)
- Door sash trim (see page 20-12)

2. Detach the door weatherstrip clip (A), then remove the door upper seal (B).

   Fastener Location
   A : Clip, 1

3. Install the seal in the reverse order of removal, and note these items:
   - Replace the clip if it's damaged.
   - Make sure the upper seal is installed in the holder (C) securely.
   - Check for water leaks (see step 7 on page 20-25).

NOTE:

- Take care not to scratch the door.
- Use a clip remover to remove the clips.

1. Detach the clips, then remove the door side sill seal (A).

   Fastener Locations
   : Clip, 8

2. Install the seal in the reverse order of removal, and replace any damaged clips.