## Charging System

#### Alternator Overhaul (cont'd)

4-34

Stator Test

20. Check that there is continuity between each pair of leads (A).

- If there is continuity, go to step 21.
- If there is no continuity, replace the alternator.

21. Check for no continuity between each lead and the coil core (B).

- If there is no continuity, go to step 22.
- If there is continuity, replace the alternator.

22. Assemble the alternator in reverse order of disassembly, and note these items:

- Be careful not to get any grease or oil on the slip rings.
- If you removed the pulley, tighten its locknut to 111 Nm (11.3 kgf/m, 81.7 lbf/ft) when you install it.

a a a