## SRS

#### DTC Troubleshooting Index (cont'd)

23-45

DTC | Detection Item | Notes
9-1 | Internal failure of the SRS unit. If intermittent, could mean internal failure of the unit or a faulty indicator light circuit. Refer to Troubleshooting Intermittent Failures (see page 23-38). | (see page 23-85)
9-2 | Internal failure of the SRS unit. If intermittent, could mean internal failure of the power supply (VB line). Refer to Troubleshooting Intermittent Failures (see page 23-38).
9-6 | Faulty left front sensor | (see page 23-88)
9-7 | Faulty right front sensor | (see page 23-91)
10-1 | Seat belt tensioners (and airbag(s)) deployed | (see page 23-85)
10-2 | Driver's side airbag deployed
10-3 | Seat belt tensioners (and airbag(s)) and driver's side airbag deployed
10-4 | Front passenger's side airbag deployed
10-5 | Seat belt tensioners (and airbag(s)) and front passenger's side airbag deployed
10-6 | Driver's and front passenger's side airbags deployed
10-7 | Seat belt tensioners (and airbag(s)) and driver's and front passenger's side airbags deployed
11-1 | Open or increased resistance in driver's side airbag inflator | (see page 23-94)
11-3 | Short to another wire or decreased resistance in driver's side airbag inflator | (see page 23-95)
11-4 | Short to power in driver's side airbag inflator | (see page 23-97)
11-5 | Short to ground in driver's side airbag inflator | (see page 23-98)
12-1 | Open or increased resistance in front passenger's side airbag inflator | (see page 23-106)
12-3 | Short to another wire or decreased resistance in front passenger's side airbag inflator | (see page 23-107)
12-4 | Short to power in front passenger's side airbag inflator | (see page 23-109)
12-5 | Short to ground in front passenger's side airbag inflator | (see page 23-110)
13-1 | Internal failure of the driver's side impact sensor | (see page 23-86)
13-2
13-3 | No signal from the driver's side impact sensor | (see page 23-118)
13-4 | Faulty power supply to the driver's side impact sensor | (see page 23-119)
14-1 | Internal failure of the front passenger's side impact sensor | (see page 23-86)
14-2
14-3 | No signal from the front passenger's side impact sensor | (see page 23-124)
14-4 | Faulty power supply to the front passenger's side impact sensor | (see page 23-125)
15-1 | Faulty OPDS unit | (see page 23-130)
15-2 | Faulty side airbag indicator light circuit | (see page 23-134)
15-3 | Faulty OPDS sensor | (see page 23-144)