## Climate Control

#### In-car Temperature Sensor Replacement

21-149

4-door NOTE: LHD type is shown, RHD type is symmetrical.

1. Remove the driver's dashboard lower cover (see page 20-75).
2. Disconnect the 2P connector (A) and the air hose (B), then remove the self-tapping screws and the in-car temperature sensor (C) from the dashboard.

3. Install the sensor in the reverse order of removal. Be sure to connect the air hose securely.

5-door

1. Remove the cover (A) and the in-car temperature sensor (B) from the dashboard, then disconnect the 2P connector (C) and the air hose (D). Be careful not to damage the cover and the dashboard.

2. Install the sensor in the reverse order of removal. Be sure to connect the air hose securely.