## EPS Components

#### DTC Troubleshooting

17-74

DTC 12: Torque Sensor T/SIG

1. Clear the DTC.
2. Start the engine.
3. Wait at least 10 seconds.

Does the EPS indicator come on?

YES - Go to step 4.

NO - The system is OK at this time.

4. Stop the engine, and verify the DTC.

Is DTC12 indicated?

YES - Go to step 5.

NO - Perform the appropriate troubleshooting for the code indicated.

5. Make sure the ignition switch is OFF, then disconnect the EPS control unit connector C (20P) and the torque sensor 6P connector.

EPS CONTROL UNIT CONNECTOR C (20P)

Wire side of female terminals

6. Check for continuity between the EPS control unit connector C (20P) terminal No. 15 and body ground.

Is there continuity?

YES - Repair short to body ground in the wire between the torque sensor and EPS control unit.

NO - Go to step 7.