## PGM-FI System

#### MIL Circuit Troubleshooting (cont'd)

11-61

33. Turn the ignition switch OFF.

34. Measure voltage between ECM/PCM connector terminal E7 and body ground.

ECM/PCM CONNECTOR E (31P)

Wire side of female terminals

Is there battery voltage?

YES - Go to step 38.

NO - Go to step 35.

35. Remove the PGM-FI main relay 1 (A).

LHD model:

RHD model:

36. Measure voltage between the PGM-FI main relay 1 4P connector terminal No. 4 and body ground.

Wire side of female terminals

Is there battery voltage?

YES - Go to step 37.

NO - Repair open in the wire between the No. 6 ECU (ECM/PCM) (15 A) fuse and the PGM-FI main relay 1.

37. Check for continuity between the PGM-FI main relay 1 4P connector terminal No. 3 and ECM/PCM connector terminal E7.

Wire side of female terminals

Is there continuity?

YES - Test the PGM-FI main relay 1, refer to the '01 Civic Shop Manual on this CD (see page 22-80). If the relay is OK, substitute a known-good ECM/PCM and recheck, refer to the '01 Civic Shop Manual on this CD (see page 11-6). If symptom/indication goes away, replace the original ECM/PCM.

NO - Repair open in the wire between the PGM-FI main relay 1 and the ECM/PCM (E7).