## Cylinder Head

#### Cam Chain Removal (cont'd)

6-14

1. Disconnect the CKP sensor connector (A) and VTC oil control solenoid valve connector (B).

1. Remove the VTC oil control solenoid valve (see page 11-107).

1. Support the engine with a jack and wood block under the oil pan.

1. Remove the ground cable (A) and remove the upper bracket (B).

1. Remove the side engine mount bracket.

1. Remove the chain case.

a a a