## SRS

#### DTC Troubleshooting - with Side Airbags (cont'd)

23-133

23. Disconnect the F1o connector (A) from the under-dash fuse/relay box (B).

24. Reconnect the negative battery cable.
25. Turn the ignition switch ON (II).

26. Check for voltage between the No. 3 terminal of the U2o connector and body ground. There should be 0.5 V or less.

U2o CONNECTOR

Wire side of female terminals

Is the voltage as specified?

YES - Faulty OPDS unit or SRS unit. Replace the OPDS unit. If the problem is still present, replace the SRS unit.

NO - Short to power in the floor wire harness or in the OPDS unit harness; replace the faulty harness.