## Standards and Service Limits

#### Engine Lubrication

2-4

Item | Measurement | Qualification | Standard or New | Service Limit
Engine oil | Capacity |  | 5.75 l (6.08 US qt, 5.06 lmp qt) | –
Oil pump | Inner-to-outer rotor clearance |  | 0.13 – 0.15 mm (0.005 – 0.006 in.) | 0.20 mm (0.008 in.)
Outer rotor-to-cylinder block clearance |  | 0.24 – 0.36 mm (0.009 – 0.014 in.) | 0.40 mm (0.016 in.)
Oil pump-to-cylinder block axial clearance |  | 0.035 – 0.100 mm (0.0014 – 0.0039 in.) | 0.15 mm (0.006 in.)
Oil pressure with oil temperature at 80°C (176°F) | At idle | 127 kPa (1.3 kgf/cm2, 18 psi) | –

Cooling

Item | Measurement | Qualification | Standard or New | Service Limit
Thermostat | Opening temperature | Begins to open | 83 – 87°C (181 – 189°F) | –
Fully open | 100°C (212°F) | –
Valve lift at fully open |  | 8.0 mm (0.31 in.) min. |

Fuel and Emissions

Item | Measurement | Qualification | Standard or New | Service Limit
Fuel tank | Capacity |  | 50 l (13.2 US gal, 11.0 lmp gal) |
Engine idle |  |  | 850 rpm (min-1) | +50 rpm (min-1)

Clutch

Item | Measurement | Qualification | Standard or New | Service Limit
Clutch disc | Rivet depth | – | 0.87 mm (0.034 in.) or more | 0.22 mm (0.009 in.)
Pressure plate | Height of diaphragm spring |  | – | 1.0 mm (0.039 in.) or less

a a a