## Fuel Supply System

#### Fuel Gauge Sending Unit Test (cont'd)

11-442

10. Relieve the fuel pressure (see page 11-430).
11. Remove the fuel fill cap.
12. Remove the rear seat cushion (see page 20-237).
13. Remove the access panel (A) from the floor.

14. Disconnect the fuel pump 5P connector (B).
15. Disconnect the quick-connect fittings from the fuel pump.
16. Using the tool, loosen the fuel tank unit locknut (A).

17. Measure the resistance between the No. 1 and No. 2 terminals with the float at E (EMPTY), 1/2 (HALF FULL), and F (FULL) positions.

If you do not get the following readings, replace the fuel gauge sending unit (see page 11-439).

Float Position | F | 1/2 | LOW | E
Resistance (ohms) | 11-13 | 68.5-74.5 | 113.4-128 | 130-132