## Cylinder Head

#### Auto-Tensioner Removal/Installation

6-26

Removal:

1. Remove the timing belt (see page 6-18).
2. Remove the auto-tensioner.

Installation:

1. Clean the timing belt pulleys and the upper and lower covers.
2. Set the crankshaft to TDC. Align the TDC mark (A) on the timing belt drive pulley with the pointer (B) on the oil pump.

3. Clean the camshaft pulley and set it to TDC.

1. The ''UP'' mark (A) on the camshaft pulley should be at the top.
2. Align the TDC marks (B) on the camshaft pulley with the top edge of the head.