## Manual Transmission

#### Transmission Reassembly (cont'd)

13-36

1. Install the speedometer driven gear.

1. Rotating torque measurement.

1. Set the transmission as shown in the illustration.

1. Shift the transmission into neutral and measure the input shaft rotating torque.

Rotating torque:

0.4 Nm (4 kgf/m, 3.5 lbf/ft) or less

1. If the reading does not fall within the limit, reselect the shims and retest the torque.

a a a