## SRS

#### DTC Troubleshooting - with Side Airbags (cont'd)

23-143

36. Turn the ignition switch OFF.

37. Disconnect the O1i connector (A) from the OPDS unit (B).

38. Turn the ignition switch ON (II).

Does the side airbag indicator light come on?

YES - Go to step 39.

NO - Faulty OPDS unit; replace the OPDS unit.

39. Turn the ignition switch OFF.
40. Disconnect the C1 connector (A) from the gauge assembly.

41. Check resistance between the No. 15 terminal of C1 connector and body ground. There should 1 M ohm or more.

C1 CONNECTOR

Wire side of female terminals

Is the resistance as specified?

YES - Short to ground in the side airbag indicator light circuit; replace the gauge assembly.

NO - Short to ground in dashboard wire harness A, floor wire harness or OPDS unit harness; replace the faulty harness.