## Doors

#### Rear Door Weatherstrip Replacement

20-161

Rear Door Centre Seal Replacement

NOTE:

- Take care not to scratch the door.
- Use a clip remover to remove the clips.

1. At the centre pillar, remove the door stop mounting bolt (A).

   Fastener Location
   A : Bolt, 1 | B : Clip, 1 | C : Clip, 17

2. Detach the clips (C), and pull out the door weatherstrip (D) from the holder areas (E), then remove it.
3. Install the weatherstrip in the reverse order of removal and note these items:
   - Replace any damaged clips.
   - Make sure the weatherstrip is installed in the holder (F) securely.
   - Apply liquid thread lock to the door stop mounting bolt before installation.
   - Check for water leaks (see step 7 on page 20-163).

NOTE: Take care not to scratch the door.

1. Pull out the door centre seal (A), then remove it.

2. Clean the top edge of the door with a sponge dampened in alcohol.
3. Apply clear sealant (B) (Cemedine P/N 08712-0004, or equivalent) to the into the top edge of the seal as shown.
4. Align the seal with the top edge of the door, then install the seal securely.