## Design Specifications

#### (cont'd)

2-33

Item | Measurement | Qualification | Specification
HONDA MULTI MATIC TRANSMISSION (CVT) | Type |  | Electronically controlled continuously variable transmission
Primary reduction |  | Direct 1:1
Gear ratio | Low-High | 2.466-0.449
Reverse | 2.466
Final reduction | Type | Single helical gear
Gear ratio | 4.562
STEERING | Type | 4-door | Rack and pinion, with electrical power assistance/hydraulic power assistance
5-door | Rack and pinion, with electrical power assistance
Overall ratio |  | 14.49
Turns, lock-to-lock |  | 2.83
Steering wheel diameter |  | 380 mm (15.0 in.)
SUSPENSION | Type | Front (4-door) | Strut
Front (5-door) | Strut
Rear | Double wishbone
Shock absorber | Front and rear | Telescopic, hydraulic, nitrogen gas-filled
WHEEL ALIGNMENT | Camber | Front | 0°
Rear | -0°45'
Caster | Front | 1°33'
Total toe | Front | 0 mm (0 in.)
Rear | In 2 mm (1/16 in.)
BRAKE | Type of service brake | Front | Power-assisted self-adjusting ventilated disc
Rear | Power-assisted self-adjusting solid disc or drum
Type of parking brake |  | Mechanical actuating, rear wheels
Pad friction surface area | Front | 35 cm2 x 2 (5.4 sq in. x 2)
Shoe friction surface area | Rear | 67 cm2 x 2 (10.3 sq in. x 2)
TYRES (4-door and 5-door (Japan made) models) | Size of front and rear tyre (4-door) | KE (1.4S), KG (1.4S, 1.6 LS), KB, KQ (GLI), KH (EXI), KN (150I), KU (EXI), KY, KF, KV, KT models | 184/70R14 88H
KK, KX models | 185/70R14 86H M + S
KM, KP models | 185/65R15 88H
KE (1.6SE), KG (1.6LS, 1.6ES) KQ (VTI), KH (VTI), KN (170I) KU (VTI, VTI-S) models | 195/60R15 88H
Size of front and rear tyre (5-door) | KE (1.4S, 1.4LS), KT models | 185/70R14 88H
KE (1.6S, 1.6LS, 1.6ES), KQ models | 195/60R15 88H
Size of spare tyre | KQ, KN, KU, KX models | T125/70D15 95M

a a a