## Power Steering

#### Pump Overhaul

17-28

Exploded View

1. *COVER
2. *ROLL PIN
3. RUBBER SEAL

   (Black colour)

   Replace.

4. SLIPPER SEAL

   (White colour)

   Replace.

5. *OUTER CASE
6. *CAM RING
7. *VANES

   (11 Plates)

8. *ROTOR
9. *SIDE PLATE
10. O-RING

    Replace.

11. 23.8 x 2.4 mm O-RING

    Replace.

12. PUMP COVER SEAL

    Replace.

13. *PUMP HOUSING CAP

    29 Nm (3.0 kgf/m, 22 lbf/ft)

14. 12.7 x 1.8 mm O-RING

    Replace.

15. *PUMP PRELOAD SPRING
16. PULLEY NUT

    64 Nm (6.5 kgf/m, 47 lbf/ft)

17. PULLEY
18. 40 mm SNAP RING
19. BALL BEARING
20. *DRIVE SHAFT
21. PUMP COVER SEAL

    Replace.

22. 13 x 1.9 mm O-RING

    Replace.

23. INLET JOINT
24. *PRESSURE CONTROL VALVE
25. *PRESSURE CONTROL VALVE SPRING
26. 16.7 x 1.8 mm O-RING

    Replace.

27. *PRESSURE CONTROL VALVE CAP

    49 Nm (5.0 kgf/m, 36 lbf/ft)

28. 13 x 1.9 mm O-RING

    Replace.