## Air Conditioning

#### A/C Refrigerant Oil Replacement (cont'd)

21-8

NOTE: LHD type is shown, RHD type is similar.

1. Discharge hose to the compressor (6 x 1.0 mm) : 9.8 Nm (1.0 kgf/m, 7.2 lbf/ft)
2. Discharge hose to the condenser (6 x 1.0 mm) : 9.8 Nm (1.0 kgf/m, 7.2 lbf/ft)
3. Condenser line to the condenser (6 x 1.0 mm) : 9.8 Nm (1.0 kgf/m, 7.2 lbf/ft)
4. Condenser line to the receiver/dryer (6 x 1.0 mm) : 9.8 Nm (1.0 kgf/m, 7.2 lbf/ft)
5. Receiver line A to the receiver/dryer (6 x 1.0 mm) : 9.8 Nm (1.0 kgf/m, 7.2 lbf/ft)
6. Receiver line A to the receiver line B : 13 Nm (1.3 kgf/m, 9.4 lbf/ft)
7. Receiver line B and the suction line to the evaporator (6 x 1.0 mm) : 9.8 Nm (1.0 kgf/m, 7.2 lbf/ft)
8. Suction line to the suction hose : 31 Nm (3.2 kgf/m, 23 lbf/ft)
9. Suction hose to the compressor (6 x 1.0 mm) : 9.8 Nm (1.0 kgf/m, 7.2 lbf/ft)
10. Compressor to the compressor bracket (8 x .25 mm) : 25 Nm (2.5 kgf/m, 18 lbf/ft)
11. Compressor bracket to the engine block (10 x 1.5 mm) : 43 Nm (4.4 kgf/m, 32 lbf/ft)

a a a