## Driveline/Axle

#### Intermediate Shaft Reassembly (cont'd)

16-22

Special Tools Required

- Driver, 07749-0010000
- Attachment, 52 x 55 mm, 07746-0010400
- Attachment, 35 mm I.D., 07746-0030400
- Oil seal driver, 07GAD-PH70201

NOTE: Refer to the Exploded View as needed during this procedure.

1. Clean the disassembled parts with solvent and dry them with compressed air. Do not wash the rubber parts with solvent.

1. Press the intermediate shaft bearing (A) into the bearing support (B) using the special tools and a press.

1. Seat the internal snap ring into the groove of the bearing support.

1. Press the intermediate shaft (A) into the shaft bearing using the special tool and a press.

1. Seat the external snap ring (A) into the groove of the intermediate shaft (B).

a a a